## Pedestrian Speed Turnstile Gate for sale, Pedestrian Turnstile Gate Company, Pedestrian Speed Gate Factory

Only with servo motor can be named speed gate

**Advantage:**

1. Pedestrian speed gate can be installed in commercial buildings, government agencies, universities, research institutes and libraries, parks, scenic areas, playgrounds, etc.

2. Handicapped wheelchair speed lane pays attention to special need, it can be customized to 100mm for wheelchair passing.

3. Speed gate with transparent acrylic panel looks beautiful and tidy.

4.Speed gate with servo motor

|  |  |
| --- | --- |
| Size | 1400mm\*160mm\*1000mm |
| Material | 304 Stainless steel, 1.5-2.0 mm thickness |
| Arm material | Acrylic 10mm thickness |
| **Motor type** | **Servo motor ( 24/36V )** |
| Lane width | 550-850mm (can be customized) |
| Net weight | 70kg/unit |
| MCBF | >10.000.000 times |
| Signal | Dry contract |
| IR sensor | 6 pairs |
| Access speed | 40 people/min |
| Open/Close speed | 0.2sec |
| Automatic reset time after failure | 5sec (adjustable) |
| Working environment | Indoor / Outdoor (Under  shelter) |
| Temperature | -25℃ --70℃ |
| Relative humidity | <90% no condensation |