

|  |  |
| --- | --- |
| **Item** | **Specification** |
| Clear-span width | 4m |
| Eave Height | 2.47m |
| Ridge Hight | 4.28m |
| Bay Distance | 4m |
| Wind Loading | ≤120km/h |
| Minimum Tent Length | 4m |
| Roof Fixing | bar tensioning |
| Framework Profile | 48mm\*105mm\*3.5mm |
| Eave Connection | Hot dip Galvanized aluminium cube tube |
| Cover Material | PVC Knife coated nylon fabric; 750g/m2 |
|  |  |
|  |  |
|  |  |

|  |  |  |
| --- | --- | --- |
|  |  | 图片62 |







内部图


**Pagoda Tent Technical Data**

**Type：4m\*4m**



|  |
| --- |
| **Optional Accessories** |
| PVC window sidewalls  Anchoring  Rain Gutter  Lining and curtain  Glass door units  Hard walling system  Glass walling system  Transparent PVC cover and sidewall  Flooring system  Weight plate |

|  |  |
| --- | --- |
|  |  |
|  |  |



**Framework main profile dimension and use**