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[image: ]RDPDD-104H Partial Discharge Tester is a new generation digital analyzer with high performance and new technique. This product is a desktop with advantages of multi-interface, TFT LCD display, reliable system, low fault rate. There is an expert analysis system in the product to judge different discharge types correctly, it also can be used to monitor the high voltage electrical equipment such as high voltage transformers continuously online. 
This partial discharge analyzer is the dedicated product to measure and analyze the insulation ability of electrical equipment. This system adopts modern electronic and computer integrated technology with the functions of signal amplification (analog signal, electronic signal, digital signal), filtration, data sampling, data processing, figure display, test report generation automatically so that it may finish the measurement and analysis of the partial discharge. The Partial Discharge Tester applicable scope, test method, test circuit, technical performance parameters fully meet the international standard IEC 60270 Partial Discharge Measurements.
· Product features
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1. Multi signal channel, desktop, TFT LCD display, reliable system, low failure rate and strong anti-interference ability.
2. It integrates the functions of partial discharge measurement, diagnosis and online monitoring.
3. [bookmark: _GoBack]Automatically generate the test report according to the test process, and browse and print the report.
4. The redisplay sampling function can restore the saved data file into a waveform and display it on the screen.
5. 4-channel electrical signal and 4-channel optical signal input port can simultaneously measure and analyze multiple partial discharge signals.
· [bookmark: _Hlk150179693]Product specifications and technical parameters
	Technical characteristics

	Number of interfaces
	Free-running 4 interfaces

	Sampling rate
	1M. 5M. 10M selected

	Sampling accuracy
	12bit

	Range changing
	-40dB, -20dB, 0dB, 20dB, 40dB, 60dB, totally 6 types

	Measurement frequency range
	3dB bandwidth 10kHz～1MHz

	Digital filtering
	10kHz ~ 1MHz freely selected

	Program controlled filter subsection
	Low frequency: 10kHz, 20kHz, 40kHz, 80kHz
High frequency: 100kHz, 200kHz, 300kHz, 400kHz

	Nonlinear error in the range
	10%

	Measurement range
	0.1pC ~ 100,000pC

	Sensibility
	0.1pC

	Capacitance range of the measured product
	6pF ~ 250µF

	Frequency range of test power
	50 ~ 500Hz

	Display

	Display screen
	12” TFT true color touchable LCD screen

	Resolution
	1024×768

	Interface

	USB
	3 types, use of external mouse, keyboard or other USB devices.

	Power supply
	AC 230V; Frequency 50Hz; Power 300W

	Electric signal interface
	4 BNC interfaces, use of signal input.

	Optical signal interface
	4 types, use of signal input

	Network interface
	1 type

	Landing button
	External landing

	General instruction

	CPU
	Basic frequency 1.60GHz

	Ram
	2.0GB

	Hard disk
	128GB SSD

	System
	Windows Xp

	Operating environment
	Environment ambient: -10 ~ 45℃ ; Humidity: ≤95%RH

	Dimensions
	Length×width×height: 474mm × 288mm × 370mm

	Weight
	15.8kg
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