|  |  |
| --- | --- |
| **Outdoor Grid Antenna** | |
| **Model: PW0727-1825** | |
| **Features :**  1670396285056   * Elegant appearance, simple installation, stable performance. * Good performance in anti-vibration and resistant to aging. * Small size and Light weight. * Fit for Outdoor Hold Pole mounted. | |
| **Technical Specification:** | |
| Frequency | 698 ~ 960 / 1710 ~ 2700MHz |
| Bandwidth | 262 / 990MHz |
| Gain | 15/18dBi |
| VSWR | ≤1.5 |
| Max power | 100W |
| Impedance | 50Ω |
| Polarization | Vertical |
| Horizontal Beamwidth | 20°/25° |
| Vertical Beamwidth | 30°/12° |
| Front to Back Ratio | ≥30dB |
| Rated Wind Velocity | 60m/s |
| Lightning Protection | DC Ground |
| Weight | 2.8kg |
| Color | Grey |
| Dimension | 900×600×600mm |
| Connector Type | N-Female or customized |
| Ingression Grade | IP65 |
| Terminal line | white 3D-FB, L=30mm |
| Radiating Element Material | Aluminum Alloy |
| Radome Material | UV-Resistance ABS |