**Features**

The rotary pouch packing machine design is advanced, the structure is reasonable, the adjustment operation, maintenance is very convenient;

\* Servo film system positioning standards; Synchronous belt transport film, stable and reliable;

\* Automatic correction function, save time and film, improve the reliability and intelligence of the whole machine

\* With a variety of automatic alarm protection functions to minimize losses;

\* The machine is matched with the measuring device, and automatically completes the whole process of product measurement, feeding, filling and bag-making, printing date, inflation (exhaust) and finished product output.

\* Bag form: pillow bag, vertical bag, hanging hole bag.

**Specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | JL-VP520 | **Film thickness** | 0.04～0.12mm |
| **Packing speed** | 5～70bags/min | **Air consumption** | 0.8Mps，0.5m³/min |
| **Film width** | 220～520mm | **bag type** | Pillow bag, stand-up bag, hole punching bag |
| **bag size** | （W）100～250mm（L） 长80～350mm | **Dimensions** |  （L）1560×（W）1100 ×（H)）1600mm |
| **power** | Single phase 220v±5%  50～60HZ     2.2～3.9KW | **Package material** | POPP/CPP ，POPP/VMCPP ，CPP/PE，Ect |
| **Alarm** |  ①No bag and no material alarm and shutdown ②Equipment overload alarm ③Low temperrate ,no ribbon alarm |