Liquid small bag packaging machine

1. Model: KL-300Y

2. Bag type: Three sided seal

3. Sealing method: horizontal sealing stripes, vertical sealing mesh, tooth shaped cutting

4. Measurement method: piston pump, containing 30L hopper, no mixing, no heating

5. Measurement range: 50~200mL

6. Bag size: W: 30-130mm L:50-200mm

7. Packaging speed: 20-40 bags/minute

8. Cutting method: standard tooth cutting

9. Ribbon coding machine, capable of printing three lines of characters with 12 characters per line

10. Includes color code detection function

11. Includes 1 set of bag making molds

12. Voltage: 1P/220V/50HZ

13. Power: 1.5Kw

14. Equipment size: 1000 \* 850 \* 1850mm

15. Equipment weight: 260kg