**Main Machine Features**

**A.** Servo motor for film drawing down system.

**B.**Automatic film rectifying deviation function;

**C.**Famous brand PLC. Pneumatic system for vertical and horizontal sealing;

**D.**Compatible with different internal and external measuring device;

**Electric parts of the main machine**

|  |  |  |
| --- | --- | --- |
| **VP73** | | |
| Name | Brand | Producing area |
| Touch-sensitive screen | WEINVIEW | Taiwan |
| Programmer controlled system | SIEMENS | Germany |
| Servo driver | SIEMENS | Germany |
| Servo motor | SIEMENS | Germany |
| Vertical Sealing Cylinder | SMC | Japan |
| Cutter Cylinder | SMC | Japan |
| Electromagnetis valve | FESTO | Germany |
| Intermediate relay | weidmuller | Germany |
| Photoelectric eye | SICK | Germany |
| Power | SCHNEIDER | Germany |
| Solid state relay | CRYDOM | Mexico |
| Thermometer control | AUTONICS | Korea |