**Main Machine Features**

**A.** Servo motor for film drawing down system.

**B.**Automatic film rectifying deviation function;

**C.**Famous brand PLC. Pneumatic system for vertical and horizontal sealing;

**D.**Compatible with different internal and external measuring device;

**Electric parts of the main machine**

|  |
| --- |
| **VP73** |
| Name | Brand | Producing area |
| Touch-sensitive screen   | WEINVIEW         | Taiwan       |
| Programmer controlled system | SIEMENS      | Germany        |
| Servo driver | SIEMENS      | Germany        |
| Servo motor | SIEMENS      | Germany        |
| Vertical Sealing Cylinder                  | SMC | Japan |
| Cutter Cylinder | SMC | Japan　       |
| Electromagnetis valve | FESTO                        | Germany        |
| Intermediate relay        | weidmuller          | Germany     　 |
| Photoelectric eye         | SICK                    | Germany        |
| Power                          | SCHNEIDER                 | Germany  |
| Solid state relay         | CRYDOM      | Mexico |
| Thermometer control         | AUTONICS       | Korea |