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MOQ: 2000
Lite Series  1.54”   

Model: AES-0154/L  4 color is available

Minimal display: suitable for accessories, pharmaceuticals, perfumery, hygiene and beauty


[image: 1.54_副本]




Specifications

	Product Dimensions (mm*mm*mm)
	53.5*38.8*15

	Active Display Area (mm*mm)
	26.9x26.9

	Weight (g)
	22

	Case Color
	white 

	Display Size (inch)
	1.54

	Resolution (pixel)
	200*200

	DPI
	183

	Display color
	BW, BWR, BWRY

	

NFC
	1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*375mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 18,000 labels per hour





MOQ: 5000
Lite Series  2.13”

Model: AES-0213/L   4 color is available

Label with simple design. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	72.8*34.5*13

	Active Display Area (mm*mm)
	48x23.1

	Weight (g)
	33

	Case Color
	white

	Display Size (inch)
	2.13

	Resolution (pixel)
	250*122

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 18,000 labels per hour


MOQ: 5000
Lite Series  2.66”

Model: AES-0266/L   4 color is available

Label with simple design. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	90.8×42.9*13

	Active Display Area (mm*mm)
	59.5x30

	Weight (g)
	36

	Case Color
	white

	Display Size (inch)
	2.66

	Resolution (pixel)
	296*152

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour



MOQ: 5000
Lite Series  2.9”

Model: AES-0290/L    4 color is available

Label with simple design. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	90.8×42.9*13

	Active Display Area (mm*mm)
	66x28.5

	Weight (g)
	39

	Case Color
	white

	Display Size (inch)
	2.9

	Resolution (pixel)
	296*128

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour



MOQ: 5000
Lite Series  4.2”

Model: AES-0420/L

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	106*86*14.1

	Active Display Area (mm*mm)
	84x63

	Weight (g)
	83

	Case Color
	white

	Display Size (inch)
	4.2

	Resolution (pixel)
	400*300

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	3*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 9,000 labels per hour



MOQ: 2000
Lite Series  7.5”

Model: AES-0750/L

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	185*121*14

	Active Display Area (mm*mm)
	162.6x97.3

	Weight (g)
	201

	Case Color
	white

	Display Size (inch)
	7.5

	Resolution (pixel)
	800*480

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	4*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 6,000 labels per hour



MOQ: 5000
Slim Series  2.13”

Model: AES-0213/S   4 color is available

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	71*34.5*11.2

	Active Display Area (mm*mm)
	48x23.1

	Weight (g)
	32

	Case Color
	White, black

	Display Size (inch)
	2.13

	Resolution (pixel)
	250*122

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 18,000 labels per hour



MOQ: 5000
Slim Series  2.66”

Model: AES-0266/S    4 color is available

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	90.7×42.8*11.2

	Active Display Area (mm*mm)
	59.5x30

	Weight (g)
	38

	Case Color
	White

	Display Size (inch)
	2.66

	Resolution (pixel)
	296*152

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour




MOQ: 5000
Slim Series  2.9”

Model: AES-0290/S   4 color is available

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	 90*42*11.2

	Active Display Area (mm*mm)
	66x28.5

	Weight (g)
	39

	Case Color
	White, black

	Display Size (inch)
	2.9

	Resolution (pixel)
	296*128

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour



MOQ: 5000
Slim Series  4.2”

Model: AES-0420/S

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	118*83.8*11.2 

	Active Display Area (mm*mm)
	84x63

	Weight (g)
	83

	Case Color
	White, black

	Display Size (inch)
	4.2

	Resolution (pixel)
	400*300

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	3*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 9,000 labels per hour




MOQ: 5000
Slim Series  7.5”

Model: AES-0750/S

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	183*118*11.2

	Active Display Area (mm*mm)
	162.6x97.3

	Weight (g)
	201

	Case Color
	white

	Display Size (inch)
	7.5

	Resolution (pixel)
	800*480

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	4*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 6,000 labels per hour




Freezer Series  2.66”

Model: AES-0266/F

Perfect to be used in freezers.
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Specifications

	Product Dimensions (mm*mm*mm)
	85.9*41.9*9.1

	Active Display Area (mm*mm)
	59.5x30

	Weight (g)
	32

	Case Color
	White

	Display Size (inch)
	2.66

	Resolution (pixel)
	296*152

	DPI
	183

	Display color
	Black and white

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	1200mAh Polymer battery

	Changeable Battery
	Not Changeable

	Working Temperature (˚C)
	-20 C°to + 40 C°

	Working Humidity (%RH)
	30~70

	Protection Level
	IP67

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour


MOQ: 2000
Rock Series  2.13”

Model: AES-0213/R

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	71*34.5*11.2

	Active Display Area (mm*mm)
	48x23.1

	Weight (g)
	32

	Case Color
	White, black

	Display Size (inch)
	2.13

	Resolution (pixel)
	250*122

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 18,000 labels per hour



MOQ: 2000
Rock Series  2.9”

Model: AES-0290/R

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	 90*42*11.2

	Active Display Area (mm*mm)
	66x28.5

	Weight (g)
	39

	Case Color
	White, black

	Display Size (inch)
	2.9

	Resolution (pixel)
	296*128

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 15,000 labels per hour



MOQ: 2000
Rock Series  3.5”

Model: AES-0350/R   4 color is available

Slim design with protective cover. Perfect in every type of department.
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Specifications

	Product Dimensions (mm*mm*mm)
	 103.5×51×12.9

	Active Display Area (mm*mm)
	79x38

	Weight (g)
	68

	Case Color
	White, black

	Display Size (inch)
	3.5

	Resolution (pixel)
	384*184

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm


	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	2*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 12,000 labels per hour


MOQ: 2000
Rock Series  4.2”

Model: AES-0420/R

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	101*88.5*12.9

	Active Display Area (mm*mm)
	84x63

	Weight (g)
	83

	Case Color
	White, black

	Display Size (inch)
	4.2

	Resolution (pixel)
	400*300

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	4*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 9,000 labels per hour




MOQ: 2000
Rock Series  5.83”

Model: AES-0583/R

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	136*112*12.9

	Active Display Area (mm*mm)
	119x88

	Weight (g)
	105

	Case Color
	White, black

	Display Size (inch)
	5.83

	Resolution (pixel)
	648*480

	DPI
	183

	Display color
	BW, BWR, BWRY

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	4*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 9,000 labels per hour


MOQ: 2000
Rock Series  10.2”

Model: AES-0102/R

Perfect for promotion stand, fruit & vegetables and appliances section.
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Specifications

	Product Dimensions (mm*mm*mm)
	234.6×170.7×12.9

	Active Display Area (mm*mm)
	215.52*143.86

	Weight (g)
	220

	Case Color
	White, black

	Display Size (inch)
	10.2

	Resolution (pixel)
	960*640

	DPI
	183

	Display color
	BW, BWR, BWRY

	
NFC
	None

	LED Flash
	None

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	8*600mAh CR2450

	Changeable Battery
	Universal single button battery (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 6,000 labels per hour




7 color ESL  7.3”

Model: AES-0730/SC

Perfect for promotion stand, fruit & vegetables and appliances section.


[image: 7色_副本]

Specifications

	Product Dimensions (mm*mm*mm)
	183*118*11.2

	Active Display Area (mm*mm)
	160x96

	Weight (g)
	201

	Case Color
	white

	Display Size (inch)
	7.3

	Resolution (pixel)
	800*480

	DPI
	183

	Display color
	Black, White, Red, Yellow, Blue, Green, Orange

	


NFC
	
1. Complies with ISO/IEC 14443 Type A standard
2. Supports NFC NDEF data format with 200 bytes writable memory
3. Communication distance is reachable maximum 10 mm

	LED Flash
	Red, Blue, Green, Yellow, White, Cyan, Purple

	Working life
	5-10 years (2-4 updates per day)

	Battery Spec
	4*600mAh CR2450

	Changeable Battery
	Battery Pack (replaceable)

	Working Temperature (˚C)
	0~40

	Working Humidity (%RH)
	30~70

	Protection Level
	IP54

	Certiﬁcation
	ROHS,CE,FCC

	RF Wireless Communicaiton Parameters
	Working Frequency：
2402MHz ~ 2480MHz
	System Throughput：
Up to 6,000 labels per hour






ESL Gateway
Model: AES-B001
[image: 基站-YTB001-All 2]
The AES-B001 Electronic Shelf Label Control Base Station provides network access, tag communication, and update control for ESL systems. It integrates Wi-Fi, RJ45, Bluetooth, and multi-channel RF communication, supports desktop, vertical, ceiling-mounted, and other installation methods, and is suitable for retail stores, supermarket chains, warehouses, and centralized ESL management scenarios.
[image: 企业微信截图_16479172175009]
Features
Private communication protocol to ensure communication security and reduce interference;
High-speed bi-directional communication with ESL labels;
Supports Wi-Fi, RJ45 Ethernet, Bluetooth, and multi-channel RF communication;
Supports PoE, 12 V DC, and USB Type-C 5 V power input;
Compatible with PanPanTech ESL labels;
LED indicators display real-time operating status.
Hardware configuration
	[bookmark: _GoBack]AES-B001 specifications
	

	Product Dimension(mm)
	155 x 155 x 35 (L x W x T)

	Weight
	approx. 332 g

	Housing Color
	White

	Housing Material
	ABS + PC

	Mounting
	Desktop, vertical, ceiling-mounted, and other installation methods

	Main processor module
	Quad-core ARM Cortex-A35 CPU, 1 GB DDR3 RAM, 16 GB eMMC storage

	Display
	4-digit LED segment display

	Indicator LEDs
	Red: power; Yellow: operating status; Green: special status

	Power supply module
	12 V DC 1 A / USB Type-C 5 V 2 A / PoE 48 V, max. 30 W

	Network module
	Wi-Fi 2.4 GHz AP/Station; RJ45 Ethernet; BLE 5.2 private protocol

	RF module
	Four-channel RF module, two transmit channels and two receive channels

	Working Frequency
	2.4 GHz (2400 MHz - 2500 MHz), private protocol

	Communication Distance
	0-25 m in non-open environments

	Operating Current
	<350 mA

	Operating Temperature
	0 °C ~ 50 °C

	Storage Temperature
	-10 °C ~ 50 °C

	Software Support
	ESL management system / base-station control system; USB Type-C debugging
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