
100KG/h French fries complete equipment quotation

**Equipment List**

|  |  |  |  |
| --- | --- | --- | --- |
| Equipment model | Device name | Equipment pictures | Device parameters |
| SSJ-3000×600 | Lifting conveyor | 提升机 | Device Configuration:   1. Size：3000\*900\*900mm 2. Power；1.5kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| QXJ—2400 | Automatic cleaning and peeling machine | 毛辊清洗机 | Device Configuration:   1. Size：2400\*1000\*2000mm 2. Power：3kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| TXJ—2000 | Picking conveyor line | 挑选流水线 | Device Configuration:   1. Size：2000\*900\*900mm 2. Power：1.5kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| TSJ—3500 | Lifting conveyor | 7提升机.jpg | Device Configuration:   1. Size：2000\*800\*850mm 2. Power：0.55 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| BLJ-100 | Picking conveyor line | 挑选流水线 | Device Configuration:  1.Size：2000\*900\*900mm  2.Power：1.5kw  3.Material：304SUS  4.Transmission method: mesh belt transmission |
| QPJ-1000 | Slicer | 切条机 | Device Configuration:   1. Size：700\*780\*1200mm 2. Power：0.75 3. Material：304SUS |
| SSJ-2500×600 | Lifting conveyor | 7提升机.jpg | Device Configuration:   1. Size：2500\*800\*850mm 2. 功率：0.55kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| QXJ-4200 | Turbine washer |  | Device Configuration:   1. Size：5000\*1000\*1200mm 2. Power：5.5kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| SSJ-3000×600 | Conveyor |  | Device Configuration:   1. Size：2000\*800\*850mm 2. Power：0.55kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| PTJ-3500×800 | Blanching line |  | Device Configuration:   1. Size：3500\*800\*1200mm 2. Power：50kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| SSJ-4000×800 | Air knife type drain conveyor | 1545454055(1) | Device Configuration:   1. Size：6500\*1100\*1200mm 2. Power：12kw 3. Material：304SUS 4. Transmission method: mesh belt transmission |
| YF-6500×800 | Frying line | /Users/wanglongjie/Desktop/A油炸流水线/2.png2 | Device Configuration:   1. Size：6500\*1000\*2500mm 2. Power：144kw 3. Material：304SUS 4. Price includes oil filter equipment 5. Transmission method: mesh belt transmission |
| SSJ-3000×800 | Picking conveyor line | 挑选流水线 | Device Configuration:  1.Size：2000\*900\*900mm  2.Power：1.5kw  3.Material：304SUS  4.Transmission method: mesh belt transmission |