**Thermostatic** Oil Bath OB-1 OB-2

**Features:**

1. LED display.

2. Automatic protection for overheating.

3. Material: Main body is is steel plate with Baking varnish ;Internal is imported stainless steel.

4. Advanced recycle pump system ensures good evenness of temperature(OB-2).  
  
**Technical Parameters:**

|  |  |  |
| --- | --- | --- |
| Model | OB-1 | OB-2 |
| Temperature Range | RT~300℃ | |
| Temperature Fluctuation | ≤1℃ | |
| Temperature Control Precision | ≤1℃ | |
| Heating Power | 2000W | |
| Power Supply | 110V/220V±10%, 50/60Hz | |
| Circulatory System | None | Have |
| Circuation Pump Flow Rate | None | 6L/min |
| Workroom Cubage(mm³) | 280\*280\*300 | 300\*300\*280 |
| Package Size(W\*D\*H)mm | 520\*420\*400 | 710\*460\*570 |
| Gross Weight | 15kg | 33kg |