**Advantage**

1. Srong versatility: Optional different metering devices, suitable for strong versatility, for powder, high viscosity, water, granule bag production. Using servo motor double film, film position is accurate, fast and stable, can adapt to thinner or thicker roll film.

2. Smooth film release: The curve design of the film release mechanism is full of aesthetic feeling, the photoelectric induction is orderly film release, and it is not easy to deviate. The servo film transport system is accurate to ensure the accurate length of the bag, and the deviation correction function can be directly operated in the display screen to replace manual correction.

3. Exquisite bag making: the bag making machine is made of unique technology, strong and not deformed, so that the film is smooth and no scratches, so that the bag molding is very standard, and the bag size is without deviation. The horizontal sealing and longitudinal sealing are pneumatic, stable and reliable, so that the bag is tightly sealed and will not leak air. It can also be equipped with exhaust to prevent bulging. The resulting bag is beautiful and practical